Release Notes for -- Linksys SPA-2102 5.2.5

2102 -- 2 Port FXS, 2 Ethernet Interface (10/100 support)

Copyright (C) 2008 by Linksys, a Division of Cisco Systems, Inc.

All Rights Reserved.

* * * * * * * * * * IMPORTANT * * * * * * * * * * * * * * * *  *
* Use of Proprietary Information and Copyright Notice:         *
* This release note document contains proprietary information  *
* that is to be used only by Sipura Technology, Linksys(R),    *
* and Cisco Systems, Inc. customers.  Any unauthorized         *
* disclosure, copying, distribution, or use of this            *
* information is prohibited. This restriction includes         *
* ALL Internet based discussion forums, e.g. DSLreports.       *
* * * * * * * * * * * * * * * * * * * * * * * * * * * * * * *  *

========================================
	New Features
========================================
 
 - N/A

========================================
	Bug Fixes
========================================

### Since version 5.2.3 ###

 - CSCsg43804 - IP Dialing fails and unit reboots when using SIP over TCP.  
   Notes - IP dialing should not be allowed when SIP over TCP or SIP 
   over TLS because  the unit only maintains 1 static TCP connection
   with the proxy server. It does not  dynamically create a TCP 
   connect to the peer on every call. The problem is fixed by  not 
   allowing IP dialing unless SIP transport is over UDP. So attempt 
   to IP dial a peer will just fail but will not cause unit to reboot.

 - CSCsm38304 - Manual Accept Media Loopback fails.  
   Notes - An incoming call requesting media loopback test with the 
   unit may be  answered automatically without ringing, or requires 
   user to offhook the called  device when the call rings, using the 
   setting <Accept Media Loopback Request>.   In the 2nd case, the 
   unit should reply 200 OK to the call, not sending a BYE.  This 
   problem is fixed.

 - CSCsk45801 - Info page displays <Call 1 Encoder> and <Call 1 Decoder> 
   as "?" during T.38 FAX  
   Notes - Instead it should display the encoder and deocder as "T38". 
   This is fixed. 

 - CSCsm38327 - Cannot show caller-id when using <Ring9 Cadence>  
   Notes - This problem is fixed. Now caller-id can be shown for all 
   ring cadence.

 - CSCso01256 - T.38 multi-page faxes fail on certain WiMAX broadband modems.

### Since version 5.2.4 ###

- CSCso34152: DTMF strict mode does not stop all "talk-off" beeps.
   The signal level threshold for qualifying DTMF digits is set higher to prevent false DTMF detection.
 
   The recommended setting for AVT transmission is as follows:
   DTMF Tx Method: AVT
   DTMF Tx Mode: Strict
   DTMF TX Strict Hold Off time: 70